Subject: Re: Galileo Update - 04/29/93
From: simon@otago.ac.nz (The Arch-Deviant)
Organization: University of Otago, Dunedin, New Zealand
Nntp-Posting-Host: thorin.otago.ac.nz
Lines: 11

In article <29APR199321594919@kelvin.jpl.nasa.gov>, baalke@kelvin.jpl.nasa.gov (Ron Baalke) writes:
> 2.  On April 23, a cruise science Memory Readout (MRO) was performed for the
> Magnetometer (MAG) instrument.  Analysis indicates the data was received
> properly.

Am I correct in assuming that the science instruments buffer their acquired
data in onboard RAM, which is then downloaded upon receipt of the MRO command?

Simon Brady                 You don't need a lot of fancy hardware for
University of Otago         Virtual Reality - just a walkman and an
Dunedin, New Zealand        attitude
