From: guykuo@carson.u.washington.edu (Guy Kuo)
Subject: Re: cd300 question
Organization: University of Washington
Lines: 4
NNTP-Posting-Host: carson.u.washington.edu

Double speed performance from a CD drive does not require SCSI-2 interfacing.
The resultant 300 kbps speed is well within the transfer rate of an LC. In
other words, I believe you have been given incorrect information.

