From: lioness@maple.circa.ufl.edu
Subject: Re: Kubota Kenai/Denali specs
Organization: Center for Instructional and Research Computing Activities
Lines: 21
Reply-To: LIONESS@ufcc.ufl.edu
NNTP-Posting-Host: maple.circa.ufl.edu

In article <1993Apr28.151652.23080@dsd.es.com>, pmartz@dsd.es.com (Paul Martz) writes:
|>Does this mean they can either do alpha or stenciling, but not both
|>simultaneously?

I don't know the answer the to this one, although with 8-bits I would assume
that it was one or the other.

|>
|>> Stereo support	yes			yes
|>> Other:			both machines will double buffer or do
|>                                                                 ^^
|>> 				stereo output per window.  Both have an
|>> 				auxiliary video output that is RS-170A,
|>> 				NTSC, and PAL
|>Same question again, does this mean they can either do double
|>buffering or stereo, but not both simultaneously?

According to the literature, it will do quadruple buffering so that you
can have double buffered stereo output.

Brian
