From: corvus@cats.ucsc.edu (Scott Corbin Crow)
Subject: mode 13h
Organization: University of California; Santa Cruz
Lines: 7
NNTP-Posting-Host: am.ucsc.edu


Does anyone know how to access and/or display multiple pages in mode 13h
while still maintaining the 1 byte per pixel memory organization?
Examples in C or Assembly would be appreciated...
Thanks
Scott

