From: Doug_Oke@mindlink.bc.ca (Doug Oke)
Subject: Memory Access Time (Was Re: SRAM and SIMMS 4 sale)
Organization: MIND LINK! - British Columbia, Canada
Lines: 41

> ben elliston writes:
>
> Msg-ID: <734606726.AA00887@f262.n620.z3.fidonet.org>
> Posted: Mon, 12 Apr 1993 10:41:0
>
> Organization: Compact Solutions, Canberra ACT Australia
>
>  > 64k of 25ns SRAM
>
> By my way of thinking, Michael, how could this memory be static RAM if it
> has a speed rating?  I didn't think SRAM needed a refresh time.
>
> Doesn't that make it fast DRAM?

This chip would take 25ns to return valid data after being issued an address.

Refresh time (none for SRAM, as you pointed out) is a different parameter,
and is not generally referred to except by motherboard designers.
>
> Cheers,
> Ben
> ----------------------------------------------------------------------------
> --
> Ben Elliston
> Bachelor of Engineering (Computer Engineering)
> University of Canberra
>
> Email:      tp923021@jarrah.canberra.edu.au
> UUCP:       ..!uunet!munnari!sserve.adfa.oz.au!compsol!root
> FidoNet:    3:620/262
> ----------------------------------------------------------------------------
> --
> If a train station is where the train stops, what's a workstation?!
> ----------------------------------------------------------------------------
> --
>
>  * Origin: % Compact Solutions % Canberra ACT Australia % (3:620/262)


--
Doug Oke - Vancouver, Canada                  Doug_Oke@mindlink.bc.ca
