From: sorlin@magnus.acs.ohio-state.edu (Steven J Orlin)
Subject: Re: Changing oil by self.
Nntp-Posting-Host: magnusug.magnus.acs.ohio-state.edu
Organization: The Ohio State University
Lines: 22


In article <1993Apr15.193712.25996@news.cs.brandeis.edu> andyh@chaos.cs.brandei
s.edu (Andrew J. Huang) writes:
>In article <1993Apr15.020356.28944@magnus.acs.ohio-state.edu> sorlin@magnus.ac
s.ohio-state.edu (Steven J Orlin) writes:
>>I take the electrodes of the Amp/Ohm/Volt meter whatever and connect one
>>to each earlobe.  Then, symmetrically insert my fingers in each of the
>>spark plug boots. No cheating guys!  both hands must be used!
>
>I have just a couple of questions about this technique.
>
>First, what firing order should I use?  Do I start with my pointer
>finger or my pinky?  Left hand or right?

Place your hands flat on a table, and arrange the firing order from left to
right.

>And secondly, I have a 12cyl and there are two cylinders unaccounted
>for.  Any suggestions?

Well, you have friends don't you???
12 cylinders might be more excitement than one person can take....
