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Il Calculate the reliability of a system consisting of one operating unit and one identical
standby unit operating for a period of 200 hours. The failure rate (A) of each unit is 0.003

lailure per hour and the failure sensing switch reliability is 1.0.
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13. Ten components were tested for 500 hours, each V{ithin prescribed cOndifi,
Component 1 failed after 30 hours; component 2 failed after 85 hours; Component3 ey

after 220 hours; and component 4 failed after 435 hours. Determine the overall compogi,
failure rate (A) for the system. iy




