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High levels of cockpit noise in an aircraft can damage the hearing of pilots who are exposed to this hazard for many hours. Cockpit
noise in a jet aircraft is mostly due to airflow at hundreds of miles per hour. This 3 x 3 contingency table shows 61 observations of data
collected by an airline pilot using a handheld sound meter in a certain aircraft cockpit. Noise level is defined as “low&rdquo; (under 88
decibels), “medium” (88 to 91 decibels), or “high” (92 decibels or more). There are three flight phases (climb, cruise, descent).
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[ Click here for the Excel Data File

(a) Calculate the following probabilities: (Round your answers to 4 decimal places.)
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The Environmental Protection Agency (EPA) requires that cities monitor over 80 contaminants in their drinking water. Samples from the
Lake Huron Water Treatment Plant gave the results shown here. All observations were below the allowable maximum, as shown by the
reported range of contaminant levels. (presumably the mean would be the midrange).

2
points. Range Allowable
Substance Detected Maximum Origin of Substance
Chromium 0.41 to 0.60 100 Discharge from steel and pulp mills, natural erosion
Barium 0.006 to 2 Discharge from drilling wastes, metal refineries, natural
0.020 erosion
Fluoride 1.89 to 1.15 4 Natural erosion, water additive, discharge from fertilizer and

aluminum factories

For each substance, estimate the standard deviation o by assuming uniform distribution and normal distribution shown in Table 8.11in
Section 8.8. (Round your answers to 4 decimal places.)

Uniform Distribution Normal Distribution
Chromium 0.0548| @ 0.0317| @

Barium 0.004| @ 0.0022| @
Fluoride 0.0173| @ 0.01| @





