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Assume FML has poo ontactwih h recompecied y I
e mpaciod iyl was consicied 10 107 cisec prmeabiy
Hole dameter =2cm
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Inlet area of each hole = 3 in’/ift
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€03 for the final cover
Slope =4:1
Ditch il have s slope = 25 and n=0.1

- Find the required Transmissivity and ADS o the geocomposite?

15 the provided pipe’s perforation adequate? Explainyour answer

- Whatis the required spacing of the outles assuming the &* perforated
pipe should not be more than 75% ul?

" nside dameter
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Whats the anchor capaciy it
Intertace fricton angle between the FML and recompacted clay = 15 degrees
‘Cover sai unit weight = 130 pf
Required factor of safety =20








