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QUESTION 10
Fransiata the folowing English instruction into the machine language described in Appendix C. (NOTE: Your anster wil have 4 hexadecimal digits - ike 14AB. Be sure (o use capital letters.)

JUMP o the instruction at memory location 24 if the conlents ofregister 0 equals the value i register &
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Click Save and Submit to save
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Instructions

Multiple Attempts Not allowed. This test can only be taken once

Force Completion This test can be saved and resumed later

¥ Question Completion Status:

QUESTION 1

Mateh the definition on the left with the correct term on the right.
A. v contains circuitry for coordinating the machine's activities

G. v contains circuitry that performs operations on data (such as addition)

D. v a collection of wires that connects the CPU and main memory

C. v contains data storage cell that are used for temporary storage of information within the CPU

- v thefirst part of a machine instruction that indicates which operation is requested by the instruction

QUESTION 2

Which of the following serve as temporary holding places for data being manipulated by the CPU?.
program counter

A. control unit
B. operand

C. register unit
D. bus

E. op-code

F. motherboard

G.arithmetic/iogic unit
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QUESTION 3

3 1@ described in Appendix C contain the ollowing bt patters (shown in hexadecimal),
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QUESTION 5§

1 1he simple machine we discussed n cass (the
NOTE: Wnen typing in yo

@ described in Appendix C), how many memory addrossos does it take o hold a mac
ur answer, please use an integer
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value (ie.0, 1, 2, otc)
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QUESTION 8

Translate the following English instructions into the machine language described ir

LOAD register 6 with the contents of memory cell B

QUESTION 9

What s the ilustration below displaying?

1. Retrieve the next
Instruction from

memory (as indicated 2 Docode the bit pattern
by the program. in e instruction agistor
Counter) and then
ncromentthe

Program counter

3.Pertorm the action
e oy e
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the stored-program concept

il be in memory cell 00 w

en the machine halts?

Appendix C. (NOTE: Your answer will have 4 hexadecimal digits - ike 14AB. Be sure to use capitallefters.)
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