From: imj1@cunixa.cc.columbia.edu (Imad M Jureidini)
Subject: Re: Problems with Toshiba 3401 CDROM
Nntp-Posting-Host: cunixa.cc.columbia.edu
Reply-To: imj1@cunixa.cc.columbia.edu (Imad M Jureidini)
Organization: Columbia University
Lines: 22

In article <1r25nt$oa5@ratatosk.uninett.no> hktth@nho.hydro.com writes:
>In article <1993Apr20.191255.10115@news.columbia.edu>, imj1@cunixa.cc.columbia.edu (Imad M Jureidini) writes:
>|> Hi!
>|> 	I recently purchased the Toshiba 3401 CDROM.  I own an Adaptec 1542B
>|> SCSI card, and I have so far failed to get the CDROM to work under DOS.  It
>
>One of the ASPI-drivers (I think it's the ASPICD) supports a /NORST
>paramter, which means to not reset the SCSI bus when it loads. This
>fixed the problem a friend of mine was having with his adaptec+tosh 
>3401.
>
>Regards,
>
>  -Terje
It worked!!!
Thank you very much!


*******************************************************************************
* imj1@cunixa.cc.columbia.edu			    Imad "Hexabyte" Jureidini *
*     The Ultimate Knight, Grand Priest of the Secrets of the Undefined.      *
*******************************************************************************
