From: jpau@oracle.com
Subject: >> Misc. Car audio forsale <<
Nntp-Posting-Host: dvlseq.us.oracle.com
Organization: Oracle Corp., Redwood Shores CA
X-Disclaimer: This message was written by an unauthenticated user
              at Oracle Corporation.  The opinions expressed are those
              of the user and not necessarily those of Oracle.
Lines: 89

o Denon DCR 5490 (high power pull out cassette deck with CD changer control)

  Features:

  - 18 W X 4
  - Theft Prevention Chassis (pull out)
  - 24 station-presets (18 FM, 6 AM)
  - Denon Optimum Reception System IV (FM circuitry-Auto high blend and FM
    pulse noise cancellor)
  - Dolby B NR
  - Key off head release
  - Flexible fader-internal front amp to rear amp and/or internal front amp
    to internal rear amp
  - Auto reverse cassette mechanism
  - Up/down manual & seek tuning
  - Music sensor
  - Stereo/Mono (FM), local switches
  - Metal tape switch
  - DIN "E" with easy installation lock-in sleeve
  - Night illumination with dash light dimmer lead
  - Preset scan
  - CD changer control
        Random play: all of tracks on a disc
        Automatic/Manual search

  Excellent condition with Manual.

  Asking $220.00 + shipping

o Yamaha YPA-300 power amplifier (car audio)
  Features:
        - SELECTABLE 2-MODE POWER OUTPUT:
          40W x 2-ch or 90W x 1-ch - all w/ extremely low distortion (0.1% THD)
        - LOW RFI CIRCUIT effectively eliminates radio frequency interference
          which might arise from DC-DC conversion
        - FULL PROTECTION CIRCUITRY protects amplifier from potential damaged
          caused by overload, short circuiting, DC leakage, excessive heat
          or mis-wiring.
        - INPUT LEVEL ADJUSTMENT allows you to complement your system with any
          audio component
        - GOLD-PLATED RCA JACK ensures a durable, optimum contact, even under
          rugged road conditions.
        - REMOTE POWER links the entire system's ON/OFF with the cassette
          receiver's ot tuner's power switch.
        - SCREW TERMINALS allow simple wiring connections
        - POWER FUSE REPLACEMENT is a simple, one-step operation.
        - ALTERNATER NOISE REDUCTION CIRCUITRY is effectively suppressed
          during driving.
  Specifications:
    Continuous Power Output
          (per channel, 4 ohms, 2 channels driven.)
          with 0.1 % THD, 20 Hz ~ 20kHz .................35W/35W
          with 0.1 % THD, 1 kHz .........................40W/40W
          (per channel, 4 ohms, 1 channels driven.)
          with 0.1 % THD, 20 Hz ~ 20kHz ................80W(BTL)
          with 0.1 % THD, 1 kHz ........................90W(BTL)
    Speaker Impedance................................4 to 8 ohms
    Frequency Response (at 1W, 4 ohms)......10 Hz to 100 kHz (+0, -1.5dB)
    Signals-to-Noise Ratio ...............................105 dB
    Total Harmonic Distortion
        - (at 20W + 20W, 1 kHz, 4 ohms, 24 kHz, LPF)......0.005%
    Dimensions (W x H x D).....................200 x 50 x 156 mm
    Weight..........................................5 lbs. 15 oz

    List price: $250.00

    This is one of the nicest/cleanest amp that I have even owned.
    I am using two of these in my car, this is just an extra one that
    I don't really need.  If you are in the bay area, and like to listen
    to it first, let me know.

    Asking $150.00 firm + shipping (brand new in box, never been installed)


o Boston Acoustic 861 seperates (car audio speakers), 6" woofers
  with seperate tweeters and crossovers.
  Brand new in box, never been installed, $259.00 at Good Guys
  Asking $199.00 firm

o 2 8" MTX free air woofers, new in box, never been installed.
  Paid $49.00 each at Good Guys
  Asking $70.00 firm

o UNGO Box top of the line 5400 auto alarm with 2 twin-buttons remote
  (patented electronic motion/shock sensor, parking light flasher, ignition
  kill, panic mode, power door lock/unlocking control, LED flashing status
  light, arms all doors, hood and trunk, etc.)
  News in box, $180.00 firm

